Good: * Combo 3D Printer * Ankermake M5 FDM * Positron (yt) *Printers2Avoid: *Bambu *FiSun * Creality *Geeetech |**Onlaunch**: Qidi Anycubic

[If open 3dPrinter Enclosure /!\] - Past 3d Printers

Py&Bat scripts
title
6f33b454ebb59ce78fbe9b9cc1a8e68d528fe87f47fdea004f6f88106958386c13edb0b943334cea901eb7f11c890f0d07733e4f313c64b3c8f9bbd1ccc4182e9040045a4c276ac0ce3b8c2b6be8042bccd23d9917146fc55ff4b630ddd2b5dc058e4a94bbc55d3562b65e5250df95490ff6b74176b050c9e3a5e5c9870787b1b11ac314eb7625465ada52dac8dace53a730686e5e67fb685737c3f0fa4ad4f07ec196b28ed71d0a9c33eb4f46a2df52 rel
Tools
*Slicer
PrusaSlicer(Windows) - [Profile:][Kobra2][GeetechMizarM] [90° ArcOverhang postprocess] 90deg-Prusa-ini-bundle
PikaSlice(Android)
Gridspace(Web)
*CAD:
FreeCAD
TinkerCAD (online)
*Guide
Print basics
Printing Temp 215°C \ 90°C
3d print with multiple colors on a single color printer [2] Script -> Pause at height
Handpainting 3d Models [2] Acrylcolor
PrintTech: ArcOverhang (90° print)
*RelayTools:
Oct4Android
* Continuous print
OR
Beagle2 (70€)
Print Error/Issues Fixes
FixPrintBed Errors

# My models/printables

# Others models/printables